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	FEATURES
	

	· Built-in microwave heats fresh food to hot meal in 60 seconds
· Advanced water-cooling system
	· 32-inch touch screen - user friendly machine interface for easy programming, changing settings, pricing and advertising

	· Dispenses pre-packaged fresh food to microwave heating before delivery
	· Energy efficient compressor, LED lighting, advanced foam insulation technology etc.

	· Coil (conveyor belt optional) with steady crawler belt dispensing with automatic X-Y pickup delivery
	· Modular design – easy front removal of cooling unit for timely maintenance or repairs

	· Self fault-diagnostics for easy maintenance
	· Standard MDB & DEX protocol interface

	· Cryogenic preservation & ozone disinfection
	· Digital price labels allowing easy price adjustments

	· Accepts latest in cashless payment and telemetry system brands and products incl PayPassTM, payWaveTM, Android/Google PayTM, Apple PayTM etc. 
	· Uses R134a refrigerant and RoHS compliant
· Video: https://www.youtube.com/watch?v=M3ECp5f2d-Y 

	
	

	MODEL
	 CFM-4C(H32)
TOUCH SCREEN MICROWAVE & X-Y CRAWLER BELT

	Size (number of standard products wide)
	Extra Large (12)

	Outside Dimensions (w x d x h) mm
	1,220 x 1,015 x 1,945

	Net Weight/Ship Weight (kg)
	400/435

	Number Selections
	Up to 72

	Storage Capacity (number of products)
	Up to 720
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	WARRANTY
Machine:  12 months

LOCAL SUPPORT
Including unlimited over-the-phone/video support
	
	

	Payment Systems
	                                                 Coin, note/bill, credit/debit card, mobile, ID card, NFC card, RS232 etc.

	Cooling Function
	Japanese brand EmbracoTM compressor refrigeration: +1 to +55 °C (adjustable) (heating +70 °C)

	Refrigerant
	R134a

	Rated Power (Vac)/Frequency (Hz)
	220-240/50
	Power Consumption (W)
	 750 to 3,000 (220-240Vac/20A)

	
	
	
	

	Contact:
Vendpro
Unit 3, 23 Geddes Street, Balcatta, Perth, WA 6021
P: 08 9240 1333 | E: info@vendpro.com.au | W: www.vendpro.com.au
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	MicroMarket, Vending & Convenience Foodservice Solutions



TCN, one of the biggest vending machine factories in China, exports machines to more than 100 countries in America, Europe & Asia. Our standard vending machines can be upgraded to include media touch screen and/or belt conveyor elevator systems. Machines come with smart remote management capability. TCN also offers vendor system solutions.
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